Percent error = [ ( experimental value – theoretical value) / theoretical value ] x 100%

|  |  |  |
| --- | --- | --- |
| Measured (ohm’s) | Experimental(ohm’s) | Percent error |
| 67.8 | 61.90 | -8.70% |
| 214.5 | 209.05 | -2.54% |
| 997 | 968.28 | -2.88% |
| 29.40K | 45332.23 | 54.2% |
| 754K | Inf. | Inf. |

Amplifier to collect more data.